Site Suitability Scorecard

	Criterion
	Weight
	Site A score
	Site B score
	Site C score

	Distance to the centre of the service area
	3
	
	
	

	Usable lot area
	2
	
	
	

	Flood risk
	4
	
	
	

	Access from a main road
	1
	
	
	

	Weighted total  (4F + 3D + 2A + 1R)
	
	
	
	

	Suitability score  (weighted total ÷ 10)
	
	
	
	




Worked example: 
A site scoring F = 5, D = 3, A = 4, R = 4 has a weighted total of 4(5) + 3(3) + 2(4) + 1(4) = 41, and a suitability score of 41 ÷ 10 = 4.1 out of 5.

Scoring key
Convert each measurement into a score from 1 to 5.
1. Flood risk (F), weight 4: entirely outside all flood hazard areas = 5; outside the current hazard area but inside the projected 2100 hazard area = 3; inside the current flood hazard area = 1.
1. Distance to the centre of the service area (D), weight 3: 500 m or less = 5; 501–1 000 m = 4; 1 001–2 000 m = 3; 2 001–3 500 m = 2; more than 3 500 m = 1.
1. Usable lot area (A), weight 2: 5 000 m² or more = 5; 3 000–4 999 m² = 4; 1 500–2 999 m² = 3; 750–1 499 m² = 2; less than 750 m² = 1.
1. Access from a main road (R), weight 1: 100 m or less = 5; 101–300 m = 4; 301–600 m = 3; 601–1 000 m = 2; more than 1 000 m = 1.


